How to Update Settings from Configuration File

From V1.6 firmware, Git2 support update settings from configuration file. Normally after upgrade with new firmware, the settings will be reset to default. Using the configuration file to update settings, will help you to save time to recover the settings, also great help if you have multiple Git2 cameras to change setting.

1. Upgrade the firmware to the latest V1.6 version, please check below link for the V1.6 beta version.
2. Save the UICONFIG.BIN file to the SD card
3. Change the settings in UICONFIG.BIN, please only choose the options value listed in   
   “git2\_config\_options.txt” file.
4. Hold the menu and power button to power on the camera, it will automatically update the settings, after update the camera will be restarted automatically, and then you will find it use the new settings now.